# 2026.6.9 V2.3.0

## JeeHell FMGS A320 (Prepar3D) INTERFACE SUPPORT [NEW]

- Added full hardware interface support for the JeeHell A320FMGS aircraft model, covering the pedestal (PED), main instrument panel (MIP), glareshield (GLARE), overhead panel (OVHD), flight controls (sidestick / rudder pedals / nosewheel tiller / brakes) and circuit breaker (CB) panels.

- Communicates with FMGS through the JeeHell SDKPRO, and keeps an FSUIPC auxiliary channel for the few discrete commands that SDKPRO does not support (e.g. the flap handle detents).


## ToLiss A319 / A320 / A321 INTERFACE MODIFY

- Added support for the ToLiss A319 and A321 aircraft models. All three variants are now integrated into a single interface DLL (`Aircraft_ToLiss319_320_321_XPlane.dll`), and iFSim.Ready automatically detects which variant is loaded, with no manual switching required.

- Fixed an issue where `Aircraft_ToLiss319_320_321_XPlane.dll` would not automatically reconnect after X-Plane was closed and restarted.

- Fixed an issue where, with the aircraft on the ground, the pedestal trim wheel motor could be driven by mistake and even run all the way to the maximum nose-up (11UP) position. Auto-trim is now gated by the ECAM flight phase: the hardware trim wheel is driven only during the in-flight auto-trim phase, and no longer turns on the ground or during manual trimming.

- The parking brake handle in the virtual cockpit is now driven by both the hardware parking brake ON and OFF signals together, instead of by the hardware parking brake ON signal alone as before.


## Fenix A319 / A320 / A321 INTERFACE MODIFY

- Fixed an intermittent crash of iFSim.Ready caused by misaligned data received when the connection between iFSim.Ready and MSFS became abnormal or briefly dropped during flight.

- Fixed an issue where the Fenix interface module kept attempting to auto-reconnect while MSFS was not running, causing the memory usage of iFSim.Ready to grow slowly.

- Fixed an issue where the flap/slat handle detent was misidentified when the handle was moved slowly (the previous signal filtering would discard the final sample taken when the handle came to rest, leaving the detent stuck on the previous position).

- The parking brake handle in the virtual cockpit is now driven by both the hardware parking brake ON and OFF signals together, instead of by the hardware parking brake ON signal alone as before.


Note:

1. This update renames and adds Profile files: `FenixA320.xml` is renamed to `FenixA319_A320_A321.xml`, `ToLissA320.xml` is renamed to `ToLissA319_A320_A321.xml`, and `JeeHell_FMGS_A320.xml` is newly added. We strongly recommend uninstalling the previous version of iFSim.Ready before installing V2.3.0. If you have customized any profile, please back up and delete your old profile files first so that iFSim.Ready loads the latest default profile.

2. This update renames the ToLiss aircraft DLL from `Aircraft_ToLiss_320_XPlane.dll` to `Aircraft_ToLiss319_320_321_XPlane.dll`. The installer will automatically remove the legacy file.

3. To use the JeeHell FMGS A320 model, you must first install JeeHell A320FMGS and FSUIPC, then deploy the CModule (`iFSimReady_FMGS.dll`) bundled with iFSim.Ready into the FMGS Hardware Modules directory. See the accompanying setup manual for detailed steps.
